
**RSIC-WHI**

****

**1. Product Name**

●RSIC-WHI Resilient Spring Isolation Clip System

• RSIC-WHI

**2. Manufacturer**

PAC International, LLC

7260 W Azure Dr

Suite 140-213

Las Vegas, NV 89130

Phone: (866) 774-2100

Fax: (866) 649-2710

Email: [**info@pac-intl.com**](mailto:info%40pac-intl.com?subject=SpecData%20inquiry)

Web: [**www.pac-intl.com**](http://www.pac-intl.com)

1. **Product Description**

**RSIC-WHI**

The RSIC-WHI is designed for use with any wood-framed, steel-framed, or concrete ceiling system where noise control is needed. The RSIC-WHI assembly decouples and isolates the gypsum board or sheet goods from the structure increasing the acoustical performance of the system.

The RSIC-WHI stops the noise and vibrations that typically would be allowed to transfer through the structure.

Materials and Composition

The RSIC-WHI clips are composed of galvanized or aluminum-zinc coated steel and is manufactured in Canby, OR. The RSIC rubber isolators are made of natural rubber and/or manufactured rubber compound. The hanger assembly bracket shall be designed to allow up to fifteen (15) degrees of vertical alignment of the suspension member without making metal-to-metal contact between the suspension and hanger assembly members. The RSIC-WHI shall be designed with an integral isolation insert selected and spaced to support the published weight. The hanger assembly shall consist of a wire loop top and bottom separated by the isoaltor. The isolation hanger deflection shall be up to ¼”   
(6mm) at full published load.

Sizes and Weight-bearing Information

RSIC-WHI is available in 220 Lb, 145 Lb, 100 Lb, 70 Lb, 50 Lb, and 30 Lb acoustical load variations.

Load range

RSIC-WHI have a working load between the published max weight and 50% of that weight.

RSIC-WHI 30 = 15 to 30 lbs

RSIC-WHI 50 = 25 to 50 lbs

RSIC-WHI 70 = 35 to 70 lbs

RSIC-WHI 100 = 50 to 100 lbs

RSIC-WHI 145 = 72 to 145 lbs

RSIC-WHi 220 = 110 to 220 lbs

Product Limitations

For interior use only with operating temperatures of 40–100 degrees F (4.4–37.8 degrees C).

.

1. **Technical Data**

Applicable Standards

ASTM International (ASTM)

●**ASTM E90** Standard Test Method for Laboratory Measurement of Airborne Sound Transmission Loss of Building Partitions and Elements

●**ASTM E413** Classification for Rating Sound Insulation

Environmental Considerations

The RSIC-WHI may contribute to LEEDS points.

The rubber RSIC fittings can be recycled.

The steel recycled content is less than 10 percent as required for fire life and safety regulations.

**5.** **Installation**

General installation: Follow manufacturer's specific installation instructions.

●Install resilient isolators in accordance with manufacturer's instructions

●Use typical fasteners and 12 Ga hanger wire to connect ceiling to joist.

●Mechanically fasten L clip and hanger wire connected to the RSIC-WHI to structure with wire, screws, bolts or expansion anchors, dependent upon structure

●Secure hanger wire to mounting bracket, RSIC-WHI and drywall grid with a minimum of 3 turns.

●Space RSIC-WHI at maximum of 48 × 48 inches (1200 × 1200 mm) on center for ceilings.

●Do not exceed design load (pull and shear) of the stated load on each RSIC-WHI Spring Isolator.

●Flanking Noise:

• Review installation details to prevent structure-borne flanking noise

• Do not allow drywall furring channels or gypsum board to contact foreign materials, including floors, ceilings or wall framing members

●Gypsum Board:

• Install gypsum board on ceilings with a 1⁄4 inch (6 mm) gap around perimeter for acoustical sealant application or RSIC Perimeter Tape.

• Install gypsum board in accordance with ASTM C840 as specified in Section 09250

●RSIC Perimeter Tape:

• Install RSIC-Perimeter Tape to the areas where non isolated areas will abut to the RSIC-WHI ceiling system. The RSIC-Perimeter Tape is not to be penetrated by fasteners.

●Acoustical Sealant:

• Seal potential air leaks with acoustical sealant to achieve best Sound Transmission Class (STC)

• Seal electrical outlets and penetrations with acoustical sealant

• Seal over RSIC Perimeter Tape with non-hardening acoustical sealant.

●Putty Pad Sealant: Acoustically seal with putty pads, electrical boxes in ceilings in which RSIC-WHI are used

**6. Availability and Cost**

Please contact PAC International, LLC. for availability and pricing information.

**7. Warranty**

RSIC-WHI clips have no warranty.

**8. Maintenance**

No maintenance is necessary.

**9. Technical Services**

PAC International Inc. offers online product pages, installation guides, and specification sheets. Technical information can be found on the website, [**www.pac-intl.com**](http://www.pac-intl.com) or by calling 866-774-2100, ext. 101 or 801. Fire ratings, sound test assemblies, CAD drawings, assembly drawings and clip specifications are also on the website.

**10. Filing Systems**

●Additional product information is available from the manufacturer upon request